The Duesey – Specifications

Case body

Ø42mm

Sandblasted titanium grade 2

Tube for the crown in titanium grade 5

Case back

Ø33.40mm

Sandblasted titanium grade 2

Markings by deep acid etching

Limited Edition XX/50 Number Etching

Pressed on Sanfil I-ring

Bezel

Ø42mm

Snap-on system

Polished titanium grade 5

With one NBR O-ring for water-resistance

Bezel crystal

Ø37.60mm

Double domed sapphire crystal with antireflective coating on each side.

ICON logo by silver metallization.

Pressed on Hytrel I-ring for water-resistance

Case back crystal

Ø25.10mm

Flat sapphire

Crown

Ø6.50mm

Polished titanium grade 5

Lizard and circle engraved by deep etching (matte finish)

With 2 NBR O-rings for water-resistance

Movement

Dubois-Depraz automatic14400 module + ETA 2892A2 TOP base movement

Luxe version (top of bridges = perlage + snail finish; rhodium plated)

Functions

Jumping hours by disc + seconds by disc, both with custom-designed fonts/layout

Custom-made oscillating weight in tungsten alloy, rhodium plated + markings with yellow gold plating + brass applied lizard made by stamping, yellow gold finish

Dial

Polished genuine onyx stone

2 frames in polished brass with titanium-like coating

Water-resistance

5 bar = 50m

Strap

Genuine alligator leather

Turned edges, no stitching

Black calf leather lining with soft (rubber-like) touch

Length : 75mm x 120mm

Width : 22mm at the case ; 20mm at the buckle

Thickness: 3.5mm at the case ; 2mm at the buckle

7 rectangular holes

Tongue buckle

Unique design, all sandblasted titanium grade 2

MSRP

$11,500